Assignment 4

Python Programming

|  |  |
| --- | --- |
| Student Name | Vaishnavi R |
| Register Number | 720319106025 |

Solution:

Link: <https://wokwi.com/projects/348373583880258130>

#include <WiFi.h>

#include <PubSubClient.h>

WiFiClient wifiClient;

#define trigpin    18

#define echopin    5

String data3;

#define ORG "n85s56"//IBM ORGANITION ID

#define DEVICE\_TYPE "Realtime"//Device type mentioned in ibm watson IOT Platform

#define DEVICE\_ID "Water24"//Device ID mentioned in ibm watson IOT Platform

#define TOKEN "12345678"

#define speed 0.034

char server[] = ORG ".messaging.internetofthings.ibmcloud.com";

char publishTopic[] = "iot-2/evt/Data/fmt/json";

char topic[] = "iot-2/cmd/home/fmt/String";

char authMethod[] = "use-token-auth";

char token[] = TOKEN;

char clientId[] = "d:" ORG ":" DEVICE\_TYPE ":" DEVICE\_ID;

PubSubClient client(server, 1883, wifiClient);

void publishData();

String command;

String data="";

long duration;

float dist;

void setup()

{

**Serial**.begin(115200);

  wifiConnect();

  pinMode(trigpin, OUTPUT);

  pinMode(echopin, INPUT);

 mqttConnect();

}

void wifiConnect() {

**Serial**.print("Connecting to "); **Serial**.print("Wifi");

  WiFi.begin("Wokwi-GUEST", "", 6);

  while (WiFi.status() != WL\_CONNECTED) {

    delay(500);

**Serial**.print(".");

  }

**Serial**.print("WiFi connected, IP address: ");

**Serial**.println(WiFi.localIP());

}

void loop()

{

    int pulseWidth = 0;

    digitalWrite(trigpin, HIGH);

    delayMicroseconds(100);

    digitalWrite(trigpin, LOW);

    pulseWidth = pulseIn(echopin, HIGH);

**Serial**.print("AlertDistance: ");

**Serial**.println(pulseWidth/58);

  publishData();

  if (!client.loop()) {

    mqttConnect();

  }

}

void mqttConnect() {

  if (!client.connected()) {

**Serial**.print("Reconnecting MQTT client to "); **Serial**.println(server);

    while (!client.connect(clientId, authMethod, token)) {

**Serial**.print(".");

      delay(500);

    }

    initManagedDevice();

**Serial**.println();

  }

}

void initManagedDevice() {

  if (client.subscribe(topic)) {

    // Serial.println(client.subscribe(topic));

**Serial**.println("IBM subscribe to cmd OK");

  } else {

**Serial**.println("subscribe to cmd FAILED");

  }

}

void publishData()

{

  digitalWrite(trigpin,LOW);

  digitalWrite(trigpin,HIGH);

  delayMicroseconds(10);

  digitalWrite(trigpin,LOW);

  duration=pulseIn(echopin,HIGH);

  dist=duration\*speed/2;

  if(dist<100){

    String payload = "{\"Normal Distance\":";

    payload += dist;

    payload += "}";

**Serial**.print("\n");

**Serial**.print("Sending payload: ");

**Serial**.println(payload);

    if (client.publish(publishTopic, (char\*) payload.c\_str())) {

**Serial**.println("Publish OK");

    }

  }

    if(dist>101 && dist<111){

    String payload = "{\"Alert distance\":";

    payload += dist;

    payload += "}";

**Serial**.print("\n");

**Serial**.print("Sending payload: ");

**Serial**.println(payload);

     if(client.publish(publishTopic, (char\*) payload.c\_str())) {

**Serial**.println("Warning crosses 110cm -- it automaticaly of the loop");

    }else {

**Serial**.println("Publish FAILED");

    }

  }

  }

  void callback(char\* subscribeTopic, byte\* payload, unsigned int payloadLength){

**Serial**.print("callback invoked for topic:");

**Serial**.println(subscribeTopic);

  for(int i=0; i<payloadLength; i++){

    dist += (char)payload[i];

  }

**Serial**.println("data:"+ data3);


  if(data3=="lighton"){

**Serial**.println(data3);

  }

  data3="";

}



Output: <https://n85s56.internetofthings.ibmcloud.com/dashboard/devices/browse>

